IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: cd73d5ed-6b47-456a-8668-d946232a4ef6, NumberOfSaves: 23]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
Time stamp: "2024-02-07T18:30:10+01:00"
Preprocessor: "ODA SDAI 23.12"
Originating system: "Autodesk Revit 24.0.20.20 (ENU) - IFC 24.0.20.20"
Application: "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)"

People and organizations
  Person "lombem" of Organization (no name given)
  Owner history of Person "lombem" of Organization (no name given) | application "Autodesk Revit 2024 (ENU)" version "2024" identifier "Revit" by Organization "Autodesk Revit 2024 (ENU)" | change NOCHANGE | created 1707231715 (2024-02-06T15:01:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 12 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5676" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5677" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5678" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5679" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5680" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5681" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5682" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5683" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5684" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5685" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5686" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:5687" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:Level 1" | elevation 2600.
        contains 17 elements
          4 x IFCBEAM | type IFCBEAMTYPE "Concrete - Rectangular Beam:300 x 300mm BEAM" | object type "Concrete - Rectangular Beam:300 x 300mm BEAM" | names: "Concrete - Rectangular Beam:300 x 300mm BEAM:7614", "Concrete - Rectangular Beam:300 x 300mm BEAM:7669", "Concrete - Rectangular Beam:300 x 300mm BEAM:7709" (+1 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_BeamCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:180mm SLAB" | object type "Floor:180mm SLAB" | FLOOR | names: "Floor:180mm SLAB:8099" | material: layers "Floor:180mm SLAB" ("Concrete - Cast-in-Place Concrete" 180.) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8387" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8388" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8389" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8390" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8391" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8392" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8393" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8394" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8395" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8396" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8397" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:8398" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
      IFCBUILDINGSTOREY "Level 2A" | long name "Level 2A" | object type "Level:Level 1" | elevation 2779.9999999999991
      IFCBUILDINGSTOREY "Level 3" | long name "Level 3" | object type "Level:Level 1" | elevation 5380.0000000000009
        contains 12 elements
          1 x IFCSLAB | type IFCSLABTYPE "Floor:180mm SLAB" | object type "Floor:180mm SLAB" | FLOOR | names: "Floor:180mm SLAB:8408" | material: layers "Floor:180mm SLAB" ("Concrete - Cast-in-Place Concrete" 180.) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCBEAM | type IFCBEAMTYPE "Concrete - Rectangular Beam:300 x 300mm BEAM" | object type "Concrete - Rectangular Beam:300 x 300mm BEAM" | names: "Concrete - Rectangular Beam:300 x 300mm BEAM:8435", "Concrete - Rectangular Beam:300 x 300mm BEAM:8437", "Concrete - Rectangular Beam:300 x 300mm BEAM:8438" (+1 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_BeamCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:9896" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:10022" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:10123" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:10210" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:10281" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | object type "Concrete-Round-Column:300mm" | names: "Concrete-Round-Column:300mm:10352" | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCROOF | object type "Basic Roof:Roof 3" | names: "Basic Roof:Roof 3:12397" | material: layers "Basic Roof:Roof 3" ("Default Roof" 300.) | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_RoofCommon
      IFCBUILDINGSTOREY "Level 3A" | long name "Level 3A" | object type "Level:Level 1" | elevation 5559.9999999999973
      IFCBUILDINGSTOREY "Level 4" | long name "Level 4" | object type "Level:Level 1" | elevation 7560.
        contains 5 elements
          5 x IFCBEAM | type IFCBEAMTYPE "Concrete - Rectangular Beam:300 x 300mm BEAM" | object type "Concrete - Rectangular Beam:300 x 300mm BEAM" | names: "Concrete - Rectangular Beam:300 x 300mm BEAM:10786", "Concrete - Rectangular Beam:300 x 300mm BEAM:10802", "Concrete - Rectangular Beam:300 x 300mm BEAM:10821" (+2 more) | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_BeamCommon, Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam

Types
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCBEAMTYPE "Concrete - Rectangular Beam:300 x 300mm BEAM" | 13 occurrences | property sets: Pset_BeamCommon, Pset_ProductRequirements
  IFCSLABTYPE "Floor:180mm SLAB" | FLOOR | 2 occurrences | material: layers "Floor:180mm SLAB" ("Concrete - Cast-in-Place Concrete" 180.) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_SlabCommon
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements
  IFCCOLUMNTYPE "Concrete-Round-Column:300mm" | COLUMN | 1 occurrence | material: "Concrete - Cast-in-Place Concrete" | property sets: Pset_ColumnCommon, Pset_ProductRequirements

Property sets
  Pset_ProductRequirements | properties | on 30 objects (30 IFCCOLUMN) | on 30 type objects
    Category = "Structural Columns" (IFCLABEL)
  Pset_ProductRequirements | properties | on 13 objects (13 IFCBEAM) | on 1 type object
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCSLAB) | on 1 type object
    Category = "Floors" (IFCLABEL)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 2" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 2A" (IFCLABEL)
  Pset_ProductRequirements: 3 more contents on 3 objects not shown
  Pset_ColumnCommon | properties | on 15 objects (15 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete-Round-Column:300mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 15 objects (15 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete-Round-Column:300mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 30 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_QuantityTakeOff | properties | on 30 objects (30 IFCCOLUMN)
    Reference = "Concrete-Round-Column:300mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 13 objects (13 IFCBEAM)
    Reference = "Concrete - Rectangular Beam:300 x 300mm BEAM" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor:180mm SLAB" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCROOF)
    Reference = "Basic Roof:Roof 3" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 30 objects (30 IFCCOLUMN)
    Reference = "Concrete-Round-Column:300mm" (IFCLABEL)
  Pset_BeamCommon | properties | on 9 objects (9 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete - Rectangular Beam:300 x 300mm BEAM" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete - Rectangular Beam:300 x 300mm BEAM" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Concrete - Rectangular Beam:300 x 300mm BEAM" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5860. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BeamCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfBeam | properties | on 13 objects (13 IFCBEAM)
    Reference = "Concrete - Rectangular Beam:300 x 300mm BEAM" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Floor:180mm SLAB" (IFCLABEL)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor:180mm SLAB" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 55.440000000000168 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Basic Roof:Roof 3" (IFCIDENTIFIER)
    TotalArea = 68.531654182282978 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2A" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 3" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 3A" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 4" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 6 objects (6 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 4 (IFCINTEGER)
  Pset_ElementShading | properties | on 1 type object
    Roughness = 304.80000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]